
# Please make this file available to others
# by sending it to <lirc@bartelmus.de>
#
# this config file was automatically generated
# using lirc-0.9.0-pre1(default) on Thu Jun 29 00:24:26 2017
#
# contributed by darkfeather@aninix.net
#
# brand:                       LG.conf
# model no. of remote control: AKB73715608
# devices being controlled by this remote: TV
#

begin remote

  name  LASKO
  bits           16
  flags SPACE_ENC|CONST_LENGTH
  eps            30
  aeps          100

  header       9063  4496
  one           579  1673
  zero          579   546
  ptrail        580
  repeat       9066  2248
  pre_data_bits   16
  pre_data       0x20DF
  gap          108528
  toggle_bit_mask 0x0

      begin codes
          KEY_POWER                0x10EF
          KEY_VOLUMEUP             0x40BF
          KEY_VOLUMEDOWN           0xC03F
          KEY_CONFIG               0xD02F
          KEY_ENTER                0x22DD
          KEY_MUTE                 0x906F
      end codes

end remote



# Please make this file available to others
# by sending it to <lirc@bartelmus.de>
#
# this config file was automatically generated
# using lirc-0.9.0-pre1(default) on Tue May  1 06:40:29 2018
#
# contributed by
#
# brand:                       ./lasko.conf
# model no. of remote control:
# devices being controlled by this remote:
#

begin remote

  name  ./lasko.conf
  flags RAW_CODES|CONST_LENGTH
  eps            30
  aeps          100

  ptrail        413
  gap          53152

      begin raw_codes

          name KEY_POWER
             1253     391    1256     391     428    1258
             1258     424    1226     428     400    1294
              397    1307     386    1291     398    1295
              396    1264     429    1289    1230    6912
             1265     383    1264     427     388    1314
             1199     425    1230     428     396    1324
              375    1259     420    1264     423    1312
              379    1293     397    1261    1259

          name KEY_MUTE
             1266     374    1256     394     426    1256
             1259     447    1202     431     397    1294
              393    1306     388    1292     397    1318
              373    1261    1258     411     414    7771
             1261     392    1257     421     395    1268
             1247     424    1225     431     398    1292
              398    1294     397    1292     396    1307
              385    1288    1229     430     397

          name KEY_VOLUMEDOWN
             1252     395    1258     392     426    1256
             1258     393    1257     398     430    1293
              395    1296     395    1267     424    1292
             1226     432     397    1265     424    7772
             1260     392    1257     391     426    1258
             1267     386    1256     400     425    1267
              427    1300     391    1315     368    1269
             1262     487     334    1297     387

          name KEY_MOVE
             1256     394    1253     420     399    1293
             1224     391    1255     403     424    1265
              427    1282     411    1294    1224     429
              396    1292     399    1290     408    7767
             1256     391    1257     422     396    1268
             1279     393    1232     393     426    1294
              396    1263     428    1315    1226     411
              425    1235     430    1259     427

      end raw_codes

end remote

# Please make this file available to others
# by sending it to <lirc@bartelmus.de>
#
# this config file was automatically generated
# using lirc-0.9.0-pre1(default) on Thu Feb  9 18:06:50 2017
#
# contributed by
#
# brand:                       Insignia
# model no. of remote control: NS-RC4NA-14
# devices being controlled by this remote: TV
#

begin remote

  name  NS-RC4NA-14
  bits           16
  flags SPACE_ENC|CONST_LENGTH
  eps            30
  aeps          100

  header       9102  4441
  one           640  1623
  zero          640   496
  ptrail        639
  repeat       9103  2189
  pre_data_bits   16
  pre_data       0x61A0
  gap          108350
  toggle_bit_mask 0x0

      begin codes
          KEY_POWER                0xF00F
          KEY_CONFIG               0xB847
          KEY_VOLUMEUP             0x30CF
          KEY_VOLUMEDOWN           0xB04F
          KEY_MUTE                 0x708F
          KEY_ENTER                0x18E7
      end codes

end remote


